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	E.T Range and relevant Safety requirement
If in doubt, please consult MSA rulebook

	Safety Item
	Length of certificate
	14.99 > 12.00
	11.99 > 10.00
	9.99 > 9.00

	SFI Flex plate 29.1
	3 years
	
	
	X

	SFI Flex plate shield 30.1
	5 years
	
	
	X

	SFI Trans shield 4.1
	5 years if rigid, 2 years if blanket
	
	X (at 10.99)
	X

	SFI Bellhousing 6.1 or 6.3
	2 years
	
	X (or 1/4” steel plate surrounding bellhousing, 360 degrees)
	X

	SFI clutch and flywheel 1.1 or 1.2
	4 years
	
	
	X

	Prop loop
	N/A
	X (at 13.99)
	X
	X

	Neutral safety switch
	N/A
	X
	X
	X

	Auto trans reverse lockout
	N/A
	X
	X
	X

	Water catch can 
	N/A
	X
	X
	X

	SFI (or billet steel) harmonic damper
	N/A
	
	X (at 10.99)
	X

	5 point SFI or FIA harness
	2 years if SFI, 5 years if FIA
	
	X
	X

	Race suit SFI 3.2A/1
	N/A
	X
	X
	

	Race suit SFI 3.2A/5
	N/A
	
	
	X

	Gloves SFI 3.3/1
	N/A
	
	
	X (at 135 mph)

	Helmet
	Check Snell No.
	X
	X
	X

	Neck brace/Hans
	Hans: 5 years
	
	X (at 10.99)
	X

	Roll hoop 10.0 spec
	N/A
	
	X
	

	Roll cage 8.50 spec
	N/A
	
	
	X

	SFI spec Roll cage padding 
	N/A
	
	X
	X

	Head protector (headrest)
	N/A
	
	X
	X

	Window net
	N/A
	
	
	X

	Fire system
	Check system
	
	
	

	Battery cut off -
NHRA approved type only
	N/A
	X (if battery relocated)
	X (if battery relocated)
	X

	Tail light
	N/A
	X
	X
	X

	Parachute
	N/A
	
	
	X (at >149 mph)



X denotes a required item
N/A: Not Applicable
Red denotes items associated with an auto transmission
Blue denotes items associated with a manual transmission
